;===========================================================================
; 
; Windows XP (32 bit) NDIS driver INF for TOPDOG (TM) 802.11n/a/g/b Wireless
; Copyright (C) 2006 Marvell Semiconductor, Inc.
;
;=========================================================================== 
[Version] 
Signature = "$Windows NT$" 
Compatible  = 1
Class=Net
ClassGUID={4D36E972-E325-11CE-BFC1-08002BE10318} 
Provider=%MRVL% 
CatalogFile=netag3n.cat
DriverVer=05/21/2007, 3.0.1.13

;===========================================================================
; Source Media Information Sections
;===========================================================================
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
; On Marvell installation disk 1 
ag300n5.sys = 1
ag300n3.sys = 1

[DestinationDirs]
W836x_PCI.XP.CopyFiles = 12 
W836x_PCI.2K.CopyFiles = 12 
DefaultDestDir = 11

[Manufacturer] 
%MRVL%=Marvell,NTamd64,NT.5.1

[Marvell]
%BUFFALO_AMG144N.DeviceDesc%    = W836x_11abgn_PCIJ.ndi, PCI\VEN_11AB&DEV_2A0B&SUBSYS_03561154
%BUFFALO_AG300N.DeviceDesc%  	= W836x_11abgn_PCIU.ndi,  PCI\VEN_11AB&DEV_2A0B&SUBSYS_03571154
%BUFFALO_AMG300N.DeviceDesc%  	= W836x_11abgn_PCI.ndi,  PCI\VEN_11AB&DEV_2A0B&SUBSYS_035C1154

[Marvell.NT.5.1]
%BUFFALO_AMG144N.DeviceDesc%    = W836x_11abgn_PCI_XPJ.ndi, PCI\VEN_11AB&DEV_2A0B&SUBSYS_03561154
%BUFFALO_AG300N.DeviceDesc%  	= W836x_11abgn_PCI_XPU.ndi,  PCI\VEN_11AB&DEV_2A0B&SUBSYS_03571154
%BUFFALO_AMG300N.DeviceDesc%  	= W836x_11abgn_PCI_XP.ndi,  PCI\VEN_11AB&DEV_2A0B&SUBSYS_035C1154

[Marvell.NTamd64]
;Empty section

;===========================================================================
; ControlFlags section
;===========================================================================
[ControlFlags]
ExcludeFromSelect = *

;===========================================================================
;	Win XP DDInstall section
;===========================================================================
[W836x_11bgn_PCI_XP.ndi]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
DelReg		= W836x.delreg.Common
AddReg          = W836x_PCI.reg, W836x_PCI_XP.reg, W836x_11bgn.reg
CopyFiles       = W836x_PCI.XP.CopyFiles

[W836x_11abgn_PCI_XP.ndi]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
DelReg		= W836x.delreg.Common
AddReg          = W836x_PCI.reg, W836x_PCI_XP.reg, W836x_11abgn.reg, WPC4400N.reg, CBAMG300N.reg
CopyFiles       = W836x_PCI.XP.CopyFiles

[W836x_11abgn_PCI_XPJ.ndi]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
DelReg		= W836x.delreg.Common
AddReg          = W836x_PCI.reg, W836x_PCI_XP.reg, W836x_11abgn.reg, WPC4400N.reg, CBAMG144N.reg
CopyFiles       = W836x_PCI.XP.CopyFiles

[W836x_11abgn_PCI_XPU.ndi]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
DelReg		= W836x.delreg.Common
AddReg          = W836x_PCI.reg, W836x_PCI_XP.reg, W836x_11abgn.reg, WPC4400N.reg, CBAG300N.reg
CopyFiles       = W836x_PCI.XP.CopyFiles

[WPC4400NXP.ndi]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
DelReg		= W836x.delreg.Common
AddReg          = W836x_PCI.reg, W836x_PCI_XP.reg, WPC4400N.reg, W836x_11bgn.reg
CopyFiles       = W836x_PCI.XP.CopyFiles

[W836x_11bgn_PCI_XP.ndi.Services]
AddService = CBAG3N, 2, W836x_PCI_XP.Service, CommonXP.EventLog

[W836x_11abgn_PCI_XP.ndi.Services]
AddService = CBAG3N, 2, W836x_PCI_XP.Service, CommonXP.EventLog

[W836x_11abgn_PCI_XPJ.ndi.Services]
AddService = CBAG3N, 2, W836x_PCI_XP.Service, CommonXP.EventLog

[W836x_11abgn_PCI_XPU.ndi.Services]
AddService = CBAG3N, 2, W836x_PCI_XP.Service, CommonXP.EventLog

[WPC4400NXP.ndi.Services]
AddService = CBAG3N, 2, WPC4400NXP.Service, CommonXP.EventLog

;===========================================================================
; PCI Win XP registry entries
;===========================================================================
[W836x_PCI_XP.reg]
HKR, Ndi,            Service,    0, "CBAG3N"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[W836x_PCI.XP.CopyFiles]
AG300N5.sys,,,2 

[W836x_PCI_XP.Service]
DisplayName    = %W836x_PCI_XP.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\AG300N5.sys
LoadOrderGroup = NDIS

[WPC4400NXP.Service]
DisplayName    = %WPC4400NXP.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\AG300N5.sys
LoadOrderGroup = NDIS

[CommonXP.EventLog]
AddReg = CommonXP.AddEventLog.reg

[CommonXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

;===========================================================================
;	Win 2K DDInstall section
;===========================================================================
[W836x_11bgn_PCI.ndi.NT]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
DelReg		= W836x.delreg.Common
AddReg          = W836x_PCI.reg, W836x_PCI_2K.reg, W836x_PCI.devID.reg, W836x_11bgn.reg
CopyFiles       = W836x_PCI.2K.CopyFiles

[W836x_11abgn_PCI.ndi.NT]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
DelReg		= W836x.delreg.Common
AddReg          = W836x_PCI.reg, W836x_PCI_2K.reg, W836x_11abgn.reg, WPC4400N.reg, CBAMG300N.reg
CopyFiles       = W836x_PCI.2K.CopyFiles

[W836x_11abgn_PCIJ.ndi.NT]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
DelReg		= W836x.delreg.Common
AddReg          = W836x_PCI.reg, W836x_PCI_2K.reg, W836x_11abgn.reg, WPC4400N.reg, CBAMG144N.reg
CopyFiles       = W836x_PCI.2K.CopyFiles

[W836x_11abgn_PCIU.ndi.NT]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
DelReg		= W836x.delreg.Common
AddReg          = W836x_PCI.reg, W836x_PCI_2K.reg, W836x_11abgn.reg, WPC4400N.reg, CBAG300N.reg
CopyFiles       = W836x_PCI.2K.CopyFiles

[WPC4400N.ndi.NT]
; "Characteristics" is (NCF_PHYSICAL | NCF_HAS_UI)
Characteristics = 0x84 
; "BusType" is PCI or CardBus
BusType         = 5 
DelReg		= W836x.delreg.Common
AddReg          = W836x_PCI.reg, W836x_PCI_2K.reg, WPC4400N.reg, W836x_PCI.devID.reg, W836x_11bgn.reg
CopyFiles       = W836x_PCI.2K.CopyFiles

[W836x_11bgn_PCI.ndi.NT.Services]
AddService = CBAG3N, 2, W836x_PCI_2K.Service, Common.EventLog

[W836x_11abgn_PCI.ndi.NT.Services]
AddService = CBAG3N, 2, W836x_PCI_2K.Service, Common.EventLog

[W836x_11abgn_PCIJ.ndi.NT.Services]
AddService = CBAG3N, 2, W836x_PCI_2K.Service, Common.EventLog

[W836x_11abgn_PCIU.ndi.NT.Services]
AddService = CBAG3N, 2, W836x_PCI_2K.Service, Common.EventLog

[WPC4400N.ndi.NT.Services]
AddService = CBAG3N, 2, WPC4400N2K.Service, Common.EventLog

;===========================================================================
; PCI Win 2K registry entries
;===========================================================================
[W836x_PCI_2K.reg]
HKR, Ndi,            Service,    0, "CBAG3N"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[W836x_PCI.2K.CopyFiles]
AG300N3.sys,,,2 

[W836x_PCI_2K.Service]
DisplayName    = %W836x_PCI_2K.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\AG300N3.sys
LoadOrderGroup = NDIS

[WPC4400N2K.Service]
DisplayName    = %WPC4400N2K.Service.DispName%
ServiceType    = 1 ;%SERVICE_KERNEL_DRIVER%
StartType      = 3 ;%SERVICE_DEMAND_START%
ErrorControl   = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\AG300N3.sys
LoadOrderGroup = NDIS

;===========================================================================
; common section
;===========================================================================
[Common.EventLog]
AddReg = Common.AddEventLog.reg

[Common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[W836x_PCI.devID.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_11AB&DEV_2A02"

===========================================================================
; Registry Key section
;===========================================================================
[W836x.delreg.Common]
HKR, Ndi\params\AdhocGMode
HKR, Ndi\params\DefaultAdhocMediaMode
HKR,, AdhocGMode
HKR,, DefaultAdhocMediaMode

[W836x_PCI.reg]
HKR,, OpMode, 			0x00002, 0	;//STA Mode

; Mode 1 (Default)
HKR,, LED0PowerOn,		0x00002, "0101ff00"
HKR,, LED1PowerOn,		0x00002, "0102fe00"
HKR,, LED0PowerOff,		0x00002, "0101fe00"
HKR,, LED1PowerOff,		0x00002, "0102fe00"
HKR,, LED0Scan,			0x00002, "0101ff00"
HKR,, LED1Scan,			0x00002, "0102fe00"
HKR,, LED0Associated,		0x00002, "0101ff00"
HKR,, LED1Associated,		0x00002, "0102ff00"
HKR,, LED0Joined,		0x00002, "0101ff00"
HKR,, LED1Joined,		0x00002, "0102ff00"
HKR,, LED0Started,		0x00002, "0101ff00"
HKR,, LED1Started,		0x00002, "0102fe00"
HKR,, LED0Tx,			0x00002, "0101ff00"
HKR,, LED1Tx,			0x00002, "0102fe00"
HKR,, LED0Rx,			0x00002, "0101ff00"
HKR,, LED1Rx,			0x00002, "0102fe00"
HKR,, LED0TxMiddle,		0x00002, "0101ff00"
HKR,, LED1TxMiddle,		0x00002, "0102fe00"
HKR,, LED0RxMiddle,		0x00002, "0101ff00"
HKR,, LED1RxMiddle,		0x00002, "0102fe00"
HKR,, LED0TxHigh,		0x00002, "0101ff00"
HKR,, LED1TxHigh,		0x00002, "0102fe00"
HKR,, LED0RxHigh,		0x00002, "0101ff00"
HKR,, LED1RxHigh,		0x00002, "0102fe00"
HKR,, LEDOffAfterRadioOff,		0x00002, "1" 

HKR, Ndi\xparams\DesiredSSID,ParamDesc,,"%SSID%"
HKR, Ndi\xparams\DesiredSSID,default,,""
HKR, Ndi\xparams\DesiredSSID,type,,"edit" 
HKR, Ndi\xparams\DesiredSSID,LimitText,,"32"
HKR, Ndi\xparams\DesiredSSID,UpperCase,,"0" 
HKR, Ndi\xparams\DesiredSSID,Optional,,"1" 

HKR, Ndi\xparams\AuthMode,ParamDesc,,"%AuthMode%"
HKR, Ndi\xparams\AuthMode,default,,"0"
HKR, Ndi\xparams\AuthMode,type,,enum
HKR, Ndi\xparams\AuthMode\enum,"0",,"%AuthMode_Open%"
HKR, Ndi\xparams\AuthMode\enum,"1",,"%AuthMode_Shared%"

HKR, Ndi\xparams\NetworkMode,ParamDesc,,"%NetworkMode%"
HKR, Ndi\xparams\NetworkMode,default,,"1"
HKR, Ndi\xparams\NetworkMode,type,,enum
HKR, Ndi\xparams\NetworkMode\enum,"0",,"%NetworkMode_AdHoc%"
HKR, Ndi\xparams\NetworkMode\enum,"1",,"%NetworkMode_Infra%"

HKR, Ndi\params\FragThsd,  ParamDesc,0 , "%FragThsds%"
HKR, Ndi\params\FragThsd,  default, 0 , "2346"
HKR, Ndi\params\FragThsd,  min, 0 , "256"
HKR, Ndi\params\FragThsd,  max, 0 , "2346"
HKR, Ndi\params\FragThsd,  step, 0 , "1"
HKR, Ndi\params\FragThsd,  Base, 0 , "10"
HKR, Ndi\params\FragThsd,  type, 0 ,"dword"

HKR, Ndi\xparams\Channel,  ParamDesc,0 , "%Channel%"
HKR, Ndi\xparams\Channel,  default, 0 , "36"
HKR, Ndi\xparams\Channel,  min, 0 , "1"
HKR, Ndi\xparams\Channel,  max, 0 , "165"
HKR, Ndi\xparams\Channel,  step, 0 , "1"
HKR, Ndi\xparams\Channel,  Base, 0 , "10"
HKR, Ndi\xparams\Channel,  type, 0 ,"dword"

HKR, Ndi\xparams\TxAntenna,  ParamDesc,0 , "%TxAntennaStr%"
HKR, Ndi\xparams\TxAntenna,  default, 0 , "2"
HKR, Ndi\xparams\TxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\TxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\TxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\TxAntenna,  type, 0 ,"dword"

HKR, Ndi\xparams\RxAntenna,  ParamDesc,0 , "%RxAntennaStr%"
HKR, Ndi\xparams\RxAntenna,  default, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  min, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  max, 0 , "ffff"
HKR, Ndi\xparams\RxAntenna,  step, 0 , "1"
HKR, Ndi\xparams\RxAntenna,  Base, 0 , "16"
HKR, Ndi\xparams\RxAntenna,  type, 0 ,"dword"

HKR, Ndi\params\RTSThsd,  ParamDesc, 0, "%RTSThsds%"
HKR, Ndi\params\RTSThsd,  default, 0, "2346"
HKR, Ndi\params\RTSThsd,  min, 0, "0"
HKR, Ndi\params\RTSThsd,  max, 0, "2346"
HKR, Ndi\params\RTSThsd,  step, 0, "1"
HKR, Ndi\params\RTSThsd,  Base, 0, "10"
HKR, Ndi\params\RTSThsd,  type, 0, "dword"

HKR, Ndi\params\PowerMode,ParamDesc,,"%PowerMode%"
HKR, Ndi\params\PowerMode,default,,"0"
HKR, Ndi\params\PowerMode,type,,enum
HKR, Ndi\params\PowerMode\enum,"0",,"%PowerMode_CAM%"
HKR, Ndi\params\PowerMode\enum,"1",,"%PowerMode_Max%"
HKR, Ndi\params\PowerMode\enum,"2",,"%PowerMode_Fast%"

HKR, Ndi\xparams\DataRate,ParamDesc,,"%DataRate%"
HKR, Ndi\xparams\DataRate,default,,"FF"
HKR, Ndi\xparams\DataRate,type,,enum
HKR, Ndi\xparams\DataRate\enum,"FF",,"%DataRate_Auto%"
HKR, Ndi\xparams\DataRate\enum,"2",,"%DataRate_1Mbps%"
HKR, Ndi\xparams\DataRate\enum,"4",,"%DataRate_2Mbps%"
HKR, Ndi\xparams\DataRate\enum,"b",,"%DataRate_5_5Mbps%"
HKR, Ndi\xparams\DataRate\enum,"16",,"%DataRate_11Mbps%"
HKR, Ndi\xparams\DataRate\enum,"C",,"%DataRate_6Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"12",,"%DataRate_9Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"18",,"%DataRate_12Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"24",,"%DataRate_18Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"30",,"%DataRate_24Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"48",,"%DataRate_36Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"60",,"%DataRate_48Mbps%" 
HKR, Ndi\xparams\DataRate\enum,"6C",,"%DataRate_54Mbps%"

HKR, Ndi\xparams\WepStatus,ParamDesc,,"%WepStatus%"
HKR, Ndi\xparams\WepStatus,default,,"1"
HKR, Ndi\xparams\WepStatus,type,,enum
HKR, Ndi\xparams\WepStatus\enum,"0",,"%Enabled%"
HKR, Ndi\xparams\WepStatus\enum,"1",,"%Disabled%"

HKR, Ndi\params\Preamble,ParamDesc,,"%PreambleStr%"
HKR, Ndi\params\Preamble,default,,"3"
HKR, Ndi\params\Preamble,type,,enum 
HKR, Ndi\params\Preamble\enum,"1",,"%PreambleStr_Auto%"
HKR, Ndi\params\Preamble\enum,"2",,"%PreambleStr_Short%" 
HKR, Ndi\params\Preamble\enum,"3",,"%PreambleStr_Long%"

HKR,, TxWepKey, 2, "" 
HKR,, WepKey1, 2, "" 
HKR,, WepKey2, 2, "" 
HKR,, WepKey3, 2, "" 
HKR,, WepKey4, 2, "" 

HKR,, RadioOn,2, "1"

HKR,, DriverRel, 2, "12/23/2005"

;HKR, Ndi\params\EWCTurboMode,ParamDesc,,"%EWCTurboMode%"
;HKR, Ndi\params\EWCTurboMode,default,,"1"
;HKR, Ndi\params\EWCTurboMode,type,,enum 
;HKR, Ndi\params\EWCTurboMode\enum,"0",,"%Disabled%"
;HKR, Ndi\params\EWCTurboMode\enum,"1",,"%Enabled%" 

HKR, Ndi\params\Aggregation,ParamDesc,,"%Aggregation%"
HKR, Ndi\params\Aggregation,default,,"2"
HKR, Ndi\params\Aggregation,type,,enum 
HKR, Ndi\params\Aggregation\enum,"0",,"%Disabled%"
HKR, Ndi\params\Aggregation\enum,"1",,"%AMSDUEnabled_4k%" 
HKR, Ndi\params\Aggregation\enum,"2",,"%AMSDUEnabled_8k%" 
HKR, Ndi\params\Aggregation\enum,"3",,"%AMPDUEnabled%" 

HKR, Ndi\params\HTModeEnabled
HKR, Ndi\params\HTModeEnabled, ParamDesc,,"%HTModeEnabled%"
HKR, Ndi\params\HTModeEnabled, default,,"1"
HKR, Ndi\params\HTModeEnabled, type,,enum
HKR, Ndi\params\HTModeEnabled\enum,"0",,"%Disabled%" 
HKR, Ndi\params\HTModeEnabled\enum,"1",,"%Enabled%"

;HKR, Ndi\params\ChannelWidth, ParamDesc,,"%ChannelWidth%"
;HKR, Ndi\params\ChannelWidth, default,,"-1"
;HKR, Ndi\params\ChannelWidth, type,,enum
;HKR, Ndi\params\ChannelWidth\enum,"0",,"%20MHz%" 
;HKR, Ndi\params\ChannelWidth\enum,"1",,"%40MHz%"
;HKR, Ndi\params\ChannelWidth\enum,"-1",,"%Auto%"

;HKR, Ndi\params\ExtChannelOffset, ParamDesc,,"%ExtChannelOffset%"
;HKR, Ndi\params\ExtChannelOffset, default,,"-1"
;HKR, Ndi\params\ExtChannelOffset, type,,enum
;HKR, Ndi\params\ExtChannelOffset\enum,"0",,"%Below%" 
;HKR, Ndi\params\ExtChannelOffset\enum,"1",,"%Above%"
;HKR, Ndi\params\ExtChannelOffset\enum,"2",,"%None%"
;HKR, Ndi\params\ExtChannelOffset\enum,"-1",,"%Auto%"

HKR, Ndi\params\GuardInterval, ParamDesc,,"%GuardInterval%"
HKR, Ndi\params\GuardInterval, default,,"-1"
HKR, Ndi\params\GuardInterval, type,,enum
HKR, Ndi\params\GuardInterval\enum,"0",,"%LongGI%" 
HKR, Ndi\params\GuardInterval\enum,"1",,"%ShortGI%"
HKR, Ndi\params\GuardInterval\enum,"-1",,"%Auto%"

HKR, Ndi\params\RegistryMimoCfg, ParamDesc,,"%Antenna%"
HKR, Ndi\params\RegistryMimoCfg, default,,"-1"
HKR, Ndi\params\RegistryMimoCfg, type,,enum
HKR, Ndi\params\RegistryMimoCfg\enum,"0",,"%2by3%" 
HKR, Ndi\params\RegistryMimoCfg\enum,"1",,"%Antenna_A%"
HKR, Ndi\params\RegistryMimoCfg\enum,"2",,"%Antenna_B%"
HKR, Ndi\params\RegistryMimoCfg\enum,"3",,"%2by2%"
HKR, Ndi\params\RegistryMimoCfg\enum,"-1",,"%Auto%"

HKR, Ndi\params\RateAdaptMode, ParamDesc,,"%RateAdaptMode%"
HKR, Ndi\params\RateAdaptMode, default,,"0"
HKR, Ndi\params\RateAdaptMode, type,,enum
HKR, Ndi\params\RateAdaptMode\enum,"0",,"%In%" 
HKR, Ndi\params\RateAdaptMode\enum,"1",,"%Out%"

HKR, Ndi\params\CSMode, ParamDesc,,"%RangeMaximization%"
HKR, Ndi\params\CSMode, default,,"0"
HKR, Ndi\params\CSMode, type,,enum
HKR, Ndi\params\CSMode\enum,"0",,"%Conservative%" 
HKR, Ndi\params\CSMode\enum,"1",,"%Aggressive%"
HKR, Ndi\params\CSMode\enum,"2",,"%Auto%"

HKR, Ndi\params\NumTxBuffer,  ParamDesc, 0, "%NumTxBuffer%"
HKR, Ndi\params\NumTxBuffer,  default, 0, "256"
HKR, Ndi\params\NumTxBuffer,  min, 0, "16"
HKR, Ndi\params\NumTxBuffer,  max, 0, "256"
HKR, Ndi\params\NumTxBuffer,  step, 0, "1"
HKR, Ndi\params\NumTxBuffer,  Base, 0, "10"
HKR, Ndi\params\NumTxBuffer,  type, 0, "dword"

;HKR, Ndi\params\RegionCode, ParamDesc,,"%RegionCode%"
;HKR, Ndi\params\RegionCode, default,,"-1"
;HKR, Ndi\params\RegionCode, type,,enum
;HKR, Ndi\params\RegionCode\enum,"16",,"%us%" 
;HKR, Ndi\params\RegionCode\enum,"32",,"%ca%" 
;HKR, Ndi\params\RegionCode\enum,"48",,"%eu%" 
;HKR, Ndi\params\RegionCode\enum,"49",,"%es%" 
;HKR, Ndi\params\RegionCode\enum,"50",,"%fr%" 
;HKR, Ndi\params\RegionCode\enum,"64",,"%jp%" 
;HKR, Ndi\params\RegionCode\enum,"128",,"%tw%" 
;HKR, Ndi\params\RegionCode\enum,"129",,"%au%" 
;HKR, Ndi\params\RegionCode\enum,"-1",,"%Default%"

HKR, Ndi\params\IntlRoaming,ParamDesc,,"%IntlRoaming%"
HKR, Ndi\params\IntlRoaming,default,,"0"
HKR, Ndi\params\IntlRoaming,type,,enum 
HKR, Ndi\params\IntlRoaming\enum,"0",,"%Off%"
HKR, Ndi\params\IntlRoaming\enum,"1",,"%On%" 

;HKR, Ndi\params\DFS,ParamDesc,,"%DFS%"
;HKR, Ndi\params\DFS,default,,"0"
;HKR, Ndi\params\DFS,type,,enum 
;HKR, Ndi\params\DFS\enum,"0",,"%Off%"
;HKR, Ndi\params\DFS\enum,"1",,"%On%" 

HKR, Ndi\params\RadioOffDisconnected,  ParamDesc, 0, "%RadioOffDisconnected%"
HKR, Ndi\params\RadioOffDisconnected,  default, 0, "4"
HKR, Ndi\params\RadioOffDisconnected,  min, 0, "1"
HKR, Ndi\params\RadioOffDisconnected,  max, 0, "86400"
HKR, Ndi\params\RadioOffDisconnected,  step, 0, "1"
HKR, Ndi\params\RadioOffDisconnected,  Base, 0, "10"
HKR, Ndi\params\RadioOffDisconnected,  type, 0, "dword"

[W836x_11bgn.reg]
HKR, Ndi\params\AdhocCreatorMode,ParamDesc,,"%AdhocCreatorModeStr%"
HKR, Ndi\params\AdhocCreatorMode,default,,"1"
HKR, Ndi\params\AdhocCreatorMode,type,,enum 
HKR, Ndi\params\AdhocCreatorMode\enum,"0",,"%AdhocCreatorModeStr_11g%"
HKR, Ndi\params\AdhocCreatorMode\enum,"1",,"%AdhocCreatorModeStr_11b%" 
HKR, Ndi\params\AdhocCreatorMode\enum,"3",,"%AdhocCreatorModeStr_11n_24GHz%"

[W836x_11abgn.reg]
HKR, Ndi\params\AdhocCreatorMode,ParamDesc,,"%AdhocCreatorModeStr%"
HKR, Ndi\params\AdhocCreatorMode,default,,"1"
HKR, Ndi\params\AdhocCreatorMode,type,,enum 
HKR, Ndi\params\AdhocCreatorMode\enum,"0",,"%AdhocCreatorModeStr_11g%"
HKR, Ndi\params\AdhocCreatorMode\enum,"1",,"%AdhocCreatorModeStr_11b%" 
HKR, Ndi\params\AdhocCreatorMode\enum,"2",,"%AdhocCreatorModeStr_11a%"
HKR, Ndi\params\AdhocCreatorMode\enum,"3",,"%AdhocCreatorModeStr_11n_24GHz%"
HKR, Ndi\params\AdhocCreatorMode\enum,"4",,"%AdhocCreatorModeStr_11n_5GHz%"

[CBAMG300N.reg]
HKR, Ndi\params\EWCTurboMode,ParamDesc,,"%EWCTurboMode%"
HKR, Ndi\params\EWCTurboMode,default,,"0"
HKR, Ndi\params\EWCTurboMode,type,,enum 
HKR, Ndi\params\EWCTurboMode\enum,"0",,"%Disabled%"
HKR, Ndi\params\EWCTurboMode\enum,"1",,"%Enabled%" 

HKR, Ndi\params\ChannelWidth, ParamDesc,,"%ChannelWidth%"
HKR, Ndi\params\ChannelWidth, default,,"0"
HKR, Ndi\params\ChannelWidth, type,,enum
HKR, Ndi\params\ChannelWidth\enum,"0",,"%20MHz%" 
HKR, Ndi\params\ChannelWidth\enum,"1",,"%40MHz%"
HKR, Ndi\params\ChannelWidth\enum,"-1",,"%Auto%"

HKR, Ndi\params\ExtChannelOffset, ParamDesc,,"%ExtChannelOffset%"
HKR, Ndi\params\ExtChannelOffset, default,,"-1"
HKR, Ndi\params\ExtChannelOffset, type,,enum
HKR, Ndi\params\ExtChannelOffset\enum,"0",,"%Below%" 
HKR, Ndi\params\ExtChannelOffset\enum,"1",,"%Above%"
HKR, Ndi\params\ExtChannelOffset\enum,"2",,"%None%"
HKR, Ndi\params\ExtChannelOffset\enum,"-1",,"%Auto%"

HKR, , RegionCode, 0, "-1"
HKR, , DFS, 0, "0"
HKR,, SSIDScanOnce,2, "1"

[CBAMG144N.reg]
HKR, Ndi\params\EWCTurboMode,ParamDesc,,"%EWCTurboMode%"
HKR, Ndi\params\EWCTurboMode,default,,"0"
HKR, Ndi\params\EWCTurboMode,type,,enum 
HKR, Ndi\params\EWCTurboMode\enum,"0",,"%Disabled%"
HKR, Ndi\params\EWCTurboMode\enum,"1",,"%Enabled%" 

HKR, , ChannelWidth, 0, "0"
HKR, , RegionCode, 0, "-1"
HKR, , DFS, 0, "0"
HKR,, SSIDScanOnce,2, "1"

[CBAG300N.reg]
HKR, Ndi\params\EWCTurboMode,ParamDesc,,"%EWCTurboMode%"
HKR, Ndi\params\EWCTurboMode,default,,"0"
HKR, Ndi\params\EWCTurboMode,type,,enum 
HKR, Ndi\params\EWCTurboMode\enum,"0",,"%Disabled%"
HKR, Ndi\params\EWCTurboMode\enum,"1",,"%Enabled%" 

HKR, Ndi\params\ChannelWidth, ParamDesc,,"%ChannelWidth%"
HKR, Ndi\params\ChannelWidth, default,,"-1"
HKR, Ndi\params\ChannelWidth, type,,enum
HKR, Ndi\params\ChannelWidth\enum,"0",,"%20MHz%" 
HKR, Ndi\params\ChannelWidth\enum,"1",,"%40MHz%"
HKR, Ndi\params\ChannelWidth\enum,"-1",,"%Auto%"

HKR, Ndi\params\ExtChannelOffset, ParamDesc,,"%ExtChannelOffset%"
HKR, Ndi\params\ExtChannelOffset, default,,"-1"
HKR, Ndi\params\ExtChannelOffset, type,,enum
HKR, Ndi\params\ExtChannelOffset\enum,"0",,"%Below%" 
HKR, Ndi\params\ExtChannelOffset\enum,"1",,"%Above%"
HKR, Ndi\params\ExtChannelOffset\enum,"2",,"%None%"
HKR, Ndi\params\ExtChannelOffset\enum,"-1",,"%Auto%"

HKR, , RegionCode, 0, "-1"
HKR, , DFS, 0, "0"
HKR,, SSIDScanOnce,2, "1"

[WPC4400N.reg]
HKR,, NoSurpriseRemoveOk, 2, "1"

;===========================================================================
; English Strings section
;===========================================================================
[Strings]
MRVL = "BUFFALO INC."
Enabled = "Enabled"
Disabled = "Disabled"
Off = "Off"
On = "On"
TxAntennaStr = "Tx Antenna Select"
RxAntennaStr = "Rx Antenna Select" 
Channel = "Channel"
FragThsds = "Fragmentation Threshold"
DataRate = "Data Rate"
DataRate_Auto = "Auto"
DataRate_1Mbps = "1 Mbps"
DataRate_2Mbps = "2 Mbps"
DataRate_5_5Mbps = "5.5 Mbps"
DataRate_11Mbps = "11 Mbps"
DataRate_6Mbps = "6 Mbps"
DataRate_9Mbps = "9 Mbps"
DataRate_12Mbps = "12 Mbps"
DataRate_18Mbps = "18 Mbps"
DataRate_24Mbps = "24 Mbps"
DataRate_36Mbps = "36 Mbps"
DataRate_48Mbps = "48 Mbps"
DataRate_54Mbps = "54 Mbps"
RTSThsds = "RTS Threshold"
AuthMode = "Authentication Mode"
AuthMode_Open = "Open"
AuthMode_Shared = "Shared"
NetworkMode = "Operation Mode"
NetworkMode_AdHoc = "Ad-Hoc"
NetworkMode_Infra = "Infrastructure"
WepStatus = "WEP Status"
SSID = "SSID"
PreambleStr = "Preamble Select"
PreambleStr_Auto = "Auto"
PreambleStr_Short = "Short Preamble"
PreambleStr_Long = "Long Preamble"
PowerMode = "Power Save Mode"
PowerMode_CAM = "CAM-Constantly Awake Mode"
PowerMode_Max = "MaxPSP-Max Power Savings"
PowerMode_Fast = "FastPSP-Fast Power Savings"
AdhocCreatorModeStr = "Adhoc Creator Mode"
AdhocCreatorModeStr_11b = "11b"
AdhocCreatorModeStr_11g = "11g"
AdhocCreatorModeStr_11a = "11a"
AdhocCreatorModeStr_11n_24GHz = "11n (2.4 GHz)"
AdhocCreatorModeStr_11n_5GHz = "11n (5 GHz)"
Aggregation = "Aggregation"
AMSDUEnabled_4k = "AMSDU Enabled (4k)" 
AMSDUEnabled_8k = "AMSDU Enabled (8k)" 
AMPDUEnabled = "AMPDU Enabled" 
EWCTurboMode = "802.11n Turbo Mode"
HTModeEnabled = "802.11n Network"
ChannelWidth = "Channel Width"
20MHz  = "20 MHz"
40MHz = "40 MHz"
Auto = "Auto"
ExtChannelOffset = "Extension Channel"
Below = "Lower"
Above = "Upper"
None = "None"
GuardInterval = "Guard Interval"
LongGI = "Standard"
ShortGI = "Short"
Antenna = "Antenna"
2by3 = "2by3"
Antenna_A = "Antenna A"
Antenna_B = "Antenna B"
2by2 = "2by2"
RateAdaptMode= "Rate adapt mode"
In = "Indoor"
Out = "Outdoor"
RangeMaximization = "Range maximization"
Conservative = "Conservative"
Aggressive = "Aggressive"
NumTxBuffer = "Number of TX Buffers"
RegionCode = "Region code"
us = "USA(FCC)"
ca = "Canada(IC)"
eu = "Europe(ETSI)"
es = "Spain"
fr = "France"
jp = "Japan(MKK)"
tw = "Taiwan(DGT)"
au = "Australia/Korea"
Default = "Default"
IntlRoaming = "Worldwide Regulatory Domain"
DFS = "802.11h DFS"
RadioOffDisconnected = "Radio Off if Disconnected"

DriverDisk = "AirNavigator CD" 

BUFFALO_AMG144N.DeviceDesc   = "BUFFALO WLI-CB-AMG144N Wireless LAN Adapter"
BUFFALO_AG300N.DeviceDesc    = "BUFFALO WLI-CB-AG300N Wireless LAN Adapter"
BUFFALO_AMG300N.DeviceDesc   = "BUFFALO WLI-CB-AMG300N Wireless LAN Adapter"
W836x_PCI_XP.Service.DispName  = "BUFFALO WLI-CB-AG300N Wireless LAN Driver Service"
W836x_PCI_2K.Service.DispName  = "BUFFALO WLI-CB-AG300N Wireless LAN Driver Service"
