;***********************************************************************
; PRISMA02.INF
;
;   PRISM 802.11 USB 2.0 Adapter installation script.
;   Installs driver, network control panel app, coinstaller, advanced properties,
;   PRISM API, and PRISM server.
;   Supports Windows 98, Me, 2000 and XP.
;   WHQL certifiable (passes INF check).
;
;   Copyright 2001-2005 Conexant Systems, Inc.  All Rights Reserved
;***********************************************************************

[Version]
 DriverVer = 06/14/2006, 3.03.41.0
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
 CatalogFile         = USB2G542.cat
 MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %A021_DESC_STR%     = PRISM_A021,        USB\VID_0411&PID_0050

;==========
[PRISM_A021]       ; Win9x
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy

[PRISM_A021.ME]    ; WinMe
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_A021.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_A021.NT]    ; Win2k and WinXP
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 BusType        = 15 ; PNP (allows USB)
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_A021.NT.Services]
 AddService= "WLI2USB2G54", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog

[PRISM_A021.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_0411&PID_0050"
;; 0x3890 = 14480 0x2280 = 8832
 HKR,,PlatformID,0,14480
 HKR,,UsbVariant,0,8832
 HKR,,VendorDesc,0,%A021_DESC_STR%
 HKR,,FWFileName,0,"PRISMA02.arm"
 
;###############################################################################
[PRISM_DRIVER_A02.Service]
 DisplayName    = %A02_SERVICE_STR%
; Description    = "%HelpText%"
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\USB2G542.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################

[COMMON_A02_DEL.reg]
 HKR,                   ,FWFileName

[COMMON_A02.reg]
 HKR,NDI                ,CardType               ,0      ,"USB"
 HKR,                   ,BusType                ,0      ,"0"  ; Inconsistency with earlier definition is needed.

[COMMON_NDIS.reg]
; Win9X
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,                   ,DeviceVxDs             ,0      ,"USB2G542.sys"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,04
 HKR,NDIS               ,MinorNdisVersion       ,1      ,00

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,                   ,DeviceVxDs             ,0      ,"USB2G542.sys"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,04
 HKR,NDIS               ,MinorNdisVersion       ,1      ,00

[COMMON_NDIS.reg.NT]
 HKR,NDI                ,Service                ,0      ,"WLI2USB2G54"
; HKR,Ndi	            ,HelpText				,0		,"%HelpText%"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
 HKR,                   ,SSID                   ,0      ,"ANY"
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,,PSMode,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,0,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,0,"enum"
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode,default,0,"1"
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode\enum,4,,%POWER_SAVE_DYNALWAYS_STR%
 HKR,NDI\params\PSMode\enum,5,,%POWER_SAVE_MAXALWAYS_STR%
 HKR,NDI\params\PSMode,optional,0,1
 
 HKR,,ConfigProfile,0,256
 HKR,NDI\params\ConfigProfile,default,0,256
 HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
 HKR,NDI\params\ConfigProfile,type,0,"enum"
 HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
 HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
 HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
 HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
 HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
 HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
 HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
 HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
 HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
 HKR,NDI\params\ConfigProfile,optional,0,1

 HKR,,NitroMode,0,"0"
 HKR,NDI\params\NitroMode,default,0,0
 HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 HKR,NDI\params\NitroMode,type,,enum
 HKR,NDI\params\NitroMode,flag,1,30,00,00,00
 HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
 HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
 HKR,NDI\params\NitroMode,optional,0,1

 HKR,,DisableQOS,0,"0"
 HKR,NDI\params\DisableQOS,default,0,0
 HKR,NDI\params\DisableQOS,ParamDesc,,%DISABLE_QOS%
 HKR,NDI\params\DisableQOS,type,,enum
 HKR,NDI\params\DisableQOS,flag,1,30,00,00,00
 HKR,NDI\params\DisableQOS\enum,0,,%NO_STR%
 HKR,NDI\params\DisableQOS\enum,1,,%YES_STR%
 HKR,NDI\params\DisableQOS,optional,0,1
 
 HKR,Ndi\params\RTSThresh,default,0,2347
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2347
 HKR,NDI\params\RTSThresh,step,0,1
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,Ndi\params\FragThresh,default,0,2346
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2346
 HKR,NDI\params\FragThresh,step,0,2
 HKR,NDI\params\FragThresh,optional,0,1
 
 HKR,,PpePdlpEnable,0,"0"
 HKR,NDI\params\PpePdlpEnable,default,0,0
 HKR,NDI\params\PpePdlpEnable,ParamDesc,,%PPE_PDLP%
 HKR,NDI\params\PpePdlpEnable,type,,enum
 HKR,NDI\params\PpePdlpEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpePdlpEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpePdlpEnable\enum,1,,%ON_STR%
 HKR,NDI\params\PpePdlpEnable,optional,0,1

 HKR,,PpeCompressEnable,0,"0"
 HKR,NDI\params\PpeCompressEnable,default,0,0
 HKR,NDI\params\PpeCompressEnable,ParamDesc,,%PPE_COMPRESS%
 HKR,NDI\params\PpeCompressEnable,type,,enum
 HKR,NDI\params\PpeCompressEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpeCompressEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpeCompressEnable\enum,1,,%ON_STR%
 HKR,NDI\params\PpeCompressEnable,optional,0,1
 
 HKR,,PpeConcatEnable,0,"0"
 HKR,NDI\params\PpeConcatEnable,default,0,0
 HKR,NDI\params\PpeConcatEnable,ParamDesc,,%PPE_CONCAT%
 HKR,NDI\params\PpeConcatEnable,type,,enum
 HKR,NDI\params\PpeConcatEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpeConcatEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpeConcatEnable\enum,1,,%ON_STR%
 HKR,NDI\params\PpeConcatEnable,optional,0,1

 HKR,,PpePiggyBackEnable,0,"0"
 HKR,NDI\params\PpePiggyBackEnable,default,0,0
 HKR,NDI\params\PpePiggyBackEnable,ParamDesc,,%PPE_PIGGYBACK%
 HKR,NDI\params\PpePiggyBackEnable,type,,enum
 HKR,NDI\params\PpePiggyBackEnable,flag,1,30,00,00,00
 HKR,NDI\params\PpePiggyBackEnable\enum,0,,%OFF_STR%
 HKR,NDI\params\PpePiggyBackEnable\enum,1,,%ON_STR%
 HKR,NDI\params\PpePiggyBackEnable,optional,0,1
 
 HKR,NDI\params\RoamingProfile,default,0,1
 HKR,NDI\params\RoamingProfile,ParamDesc,0,%ROAM_PROFILE_STR%
 HKR,NDI\params\RoamingProfile,type,0,"enum"
 HKR,NDI\params\RoamingProfile,flag,1,30,00,00,00
 HKR,NDI\params\RoamingProfile\enum,0,,%ROAM_PROFILE_SOHO%
 HKR,NDI\params\RoamingProfile\enum,1,,%ROAM_PROFILE_HIGH%
 HKR,NDI\params\RoamingProfile\enum,2,,%ROAM_PROFILE_MEDIUM%
 HKR,NDI\params\RoamingProfile\enum,3,,%ROAM_PROFILE_LOW%
 HKR,NDI\params\RoamingProfile,optional,0,1

 HKR,,11dMode,0,"0"
 HKR,NDI\params\11dMode,default,0,0
 HKR,NDI\params\11dMode,ParamDesc,0,%D_MODE_STR%
 HKR,NDI\params\11dMode,type,0,"enum"
 HKR,NDI\params\11dMode,flag,1,30,00,00,00
 HKR,NDI\params\11dMode\enum,0,,%D_MODE_NONE%
 HKR,NDI\params\11dMode\enum,1,,%D_MODE_STRICT%
 HKR,NDI\params\11dMode\enum,2,,%D_MODE_FLEXIBLE%
 HKR,NDI\params\11dMode,optional,0,1

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers

[PRISM_NDI.copy]

[PRISM_NDI.copy.ME]

[PRISM_COINSTALL.copy.NT]

[PRISM_DRIVER.copy]
 USB2G542.sys
 PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.ME]
 USB2G542.sys
 PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.NT]
 USB2G542.sys

[PRISM_APPLET.copy]

[PRISM_APPLET.copy.ME]

[PRISM_APPLET.copy.NT]

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 USB2G542.sys           = 1
 PRISMIOC.vxd           = 1

;###############################################################################
[Strings]
;String ID               = String Text
;---------                 -----------
 VER_VENDOR_STR          = "BUFFALO INC."
 VER_VENDOR_NAME_STR     = "BUFFALO INC."
 INSTALL_DISK_STR        = "AirNavigator CD"

 A021_DESC_STR           = "BUFFALO WLI2-USB2-G54 Wireless LAN Adapter"
 A02_SERVICE_STR         = "BUFFALO WLI2-USB2-G54 Wireless LAN Driver"

 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic (Auto)"
 POWER_SAVE_MAX_STR      = "Maximum (Auto)"
 POWER_SAVE_DYNALWAYS_STR= "Dynamic"
 POWER_SAVE_MAXALWAYS_STR= "Maximum"
 RTSTHRESH_STR           = "RTS Threshold"
 FRAGTHRESH_STR          = "Fragmentation Threshold"
 ON_STR                  = "On"
 OFF_STR                 = "Off"
 YES_STR                  = "Yes"
 NO_STR                 = "No"
DISABLE_QOS		 = "DisableQOS"
 CONFIG_PROFILE          = "Configuration Profile"
 CONFIG_PROF_B_ONLY      = "B only"
 CONFIG_PROF_MIXED       = "Mixed"
 CONFIG_PROF_MIXED_LONG  = "Mixed Long"
 CONFIG_PROF_G_ONLY      = "G only"
 CONFIG_PROF_TEST        = "Test"
 CONFIG_PROF_B_WIFI      = "B WiFi"
 CONFIG_PROF_MIXED_SHORT = "Mixed Short"
 CONFIG_PROF_WIFI_SPEC   = "WiFi Spec"
 NITRO_MODE              = "Nitro Mode"
 PPE_PDLP                = "Direct Link"
 PPE_COMPRESS            = "Compression"
 PPE_CONCAT              = "Concatenation"
 PPE_PIGGYBACK           = "PiggyBack"
 ROAM_PROFILE_STR        = "Roaming Profile"
 ROAM_PROFILE_SOHO       = "Single AP"
 ROAM_PROFILE_HIGH       = "High Density"
 ROAM_PROFILE_MEDIUM     = "Medium Density"
 ROAM_PROFILE_LOW        = "Low Density"
 D_MODE_STR              = "802.11d mode"
 D_MODE_NONE             = "None"
 D_MODE_STRICT           = "Strict"
 D_MODE_FLEXIBLE         = "Flexible"
