;****************************************************************************************
;
;   DR71WU.inf
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   D-Link RT73 series USB Wireless LAN Card.
;
;   Copyright (c)2005 , D-Link Corp., All Rights Reserved
;   All Rights Reserved.
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %D-Link%
Compatible      = 1
DriverVer       = 07/17/2009, 1.03.05.0000
CatalogFile     = Dr71WU.cat            ;for WHQL certified

[ControlFlags]
;***********D-Link 802.11g board  ***********
ExcludeFromSelect = VID_07D1&PID_3C0C
ExcludeFromSelect = VID_07D1&PID_3C03
ExcludeFromSelect = VID_07D1&PID_3C04
ExcludeFromSelect = VID_07D1&PID_3C07


[Manufacturer]
%D-Link%        = D-Link,NTX86, NTAMD64


[D-Link]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%DWLG122C2.DeviceDesc%      = G122C2.ndi,        USB\VID_07D1&PID_3C0C
%DWLG122C1.DeviceDesc%      = G122C1.ndi,        USB\VID_07D1&PID_3C03
%WUA1340.DeviceDesc%	    = WUA1340.ndi,       USB\VID_07D1&PID_3C04
%DWA110.DeviceDesc%	    = DWA110.ndi,        USB\VID_07D1&PID_3C07

[D-Link.NTX86]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%DWLG122C2.DeviceDesc%      = G122C2.ndi,        USB\VID_07D1&PID_3C0C
%DWLG122C1.DeviceDesc%      = G122C1.ndi,        USB\VID_07D1&PID_3C03
%WUA1340.DeviceDesc%	    = WUA1340.ndi,       USB\VID_07D1&PID_3C04
%DWA110.DeviceDesc%	    = DWA110.ndi,        USB\VID_07D1&PID_3C07

[D-Link.NTAMD64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%DWLG122C2.DeviceDesc%      = G122C2.ndi,        USB\VID_07D1&PID_3C0C
%DWLG122C1.DeviceDesc%      = G122C1.ndi,        USB\VID_07D1&PID_3C03
%WUA1340.DeviceDesc%	    = WUA1340.ndi,       USB\VID_07D1&PID_3C04
%DWA110.DeviceDesc%	    = DWA110.ndi,        USB\VID_07D1&PID_3C07

;*******************************************************************************************
; Windows 9X specific entries
;*******************************************************************************************
[G122C2.ndi]
AddReg                  = G122C29x.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[G122C1.ndi]
AddReg                  = G122C19x.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[WUA1340.ndi]
AddReg                  = WUA13409x.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

[DWA110.ndi]
AddReg                  = DWA110.ndi.reg, Common.reg, USB9X.ndi.reg
CopyFiles               = win9x.CopyFiles

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************
[G122C2.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[G122C1.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles


[WUA1340.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[DWA110.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

; NT services sections
[G122C2.ndi.NT.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

[G122C1.ndi.NT.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

[WUA1340.ndi.NT.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

[DWA110.ndi.NT.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog


;*******************************************************************************************
; NTAMD64 specific entries
;*******************************************************************************************
[G122C2.ndi.NTAMD64]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NTAMD64.CopyFiles

[G122C1.ndi.NTAMD64]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NTAMD64.CopyFiles

[WUA1340.ndi.NTAMD64]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NTAMD64.CopyFiles

[DWA110.ndi.NTAMD64]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NTAMD64.CopyFiles

; NT services sections
[G122C2.ndi.NTAMD64.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

[G122C1.ndi.NTAMD64.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

[WUA1340.ndi.NTAMD64.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

[DWA110.ndi.NTAMD64.Services]
AddService              = RT73, 2, D-Link.Service, common.EventLog

;*******************************************************************************************
; common regs for NT and W9x
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
;HKR, NDI\params\Radio,            ParamDesc,       0, %RADIO_ON_OFF%
;HKR, NDI\params\Radio,            type,            0, "enum"
;HKR, NDI\params\Radio,            default,         0, "0"
;HKR, NDI\params\Radio\enum,       1,               0, %DISABLE%
;HKR, NDI\params\Radio\enum,       0,               0, %ENABLE%

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
;HKR, NDI\params\AutoReconnect,          ParamDesc,          0, %AUTO_RECONNECT%
;HKR, NDI\params\AutoReconnect,          type,               0, "enum"
;HKR, NDI\params\AutoReconnect,          default,            0, "1"
;HKR, NDI\params\AutoReconnect\enum,     0,                  0, %DISABLE%
;HKR, NDI\params\AutoReconnect\enum,     1,                  0, %ENABLE%

;
; Country Region G Band
;
HKR, ,                                 CountryRegion,      0, "0"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, %COUNTRY_11G%
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, "0"
;HKR, NDI\params\CountryRegion\enum,    0,                  0, %CH_1-11%
;HKR, NDI\params\CountryRegion\enum,    1,                  0, %CH_1-13%
;HKR, NDI\params\CountryRegion\enum,    2,                  0, %CH_10-11%
;HKR, NDI\params\CountryRegion\enum,    3,                  0, %CH_10-13%
;HKR, NDI\params\CountryRegion\enum,    4,                  0, %CH_14%
;HKR, NDI\params\CountryRegion\enum,    5,                  0, %CH_1-14%
;HKR, NDI\params\CountryRegion\enum,    6,                  0, %CH_3-9%

;
; Country Region A Band
;
HKR, ,                                 CountryRegionABand, 0, "7"
;HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, %COUNTRY_11A%
;HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
;HKR, NDI\params\CountryRegionABand,    default,            0, "7"
;HKR, NDI\params\CountryRegionABand\enum,0,                 0, %CH_36-64_149-165%
;HKR, NDI\params\CountryRegionABand\enum,1,                 0, %CH_36-140%
;HKR, NDI\params\CountryRegionABand\enum,2,                 0, %CH_36-64%
;HKR, NDI\params\CountryRegionABand\enum,3,                 0, %CH_52-64_149-161%
;HKR, NDI\params\CountryRegionABand\enum,4,                 0, %CH_149-165%
;HKR, NDI\params\CountryRegionABand\enum,5,                 0, %CH_149-161%
;HKR, NDI\params\CountryRegionABand\enum,6,                 0, %CH_36-48%
;HKR, NDI\params\CountryRegionABand\enum,7,                 0, %CH_36-165%
;HKR, NDI\params\CountryRegionABand\enum,8,                 0, %CH_52-64%
;HKR, NDI\params\CountryRegionABand\enum,9,                 0, %CH_34-46%
;HKR, NDI\params\CountryRegionABand\enum,10,                0, %CH_34-64%

;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "3"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "1"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

; Show Hidden SSID in Site Survey Page
HKR, ,                            ShowHiddenSSID,  0, "1"   ; 0=disable(default), 1=enable

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                                  AdhocOfdm, 0, "0"
;HKR, NDI\params\AdhocOfdm,              ParamDesc, 0, %ADHOC_MODE%
;HKR, NDI\params\AdhocOfdm,              type,      0, "enum"
;HKR, NDI\params\AdhocOfdm,              default,   0, "1"
;HKR, NDI\params\AdhocOfdm\enum,         0,         0, %80211_B_ONLY%
;HKR, NDI\params\AdhocOfdm\enum,         1,         0, %80211_BG_MIX%
;HKR, NDI\params\AdhocOfdm\enum,         2,         0, %80211_G_ONLY%

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"
;HKR, NDI\params\BGProtection,           ParamDesc, 0, %BG_PROTECTION%
;HKR, NDI\params\BGProtection,           type,      0, "enum"
;HKR, NDI\params\BGProtection,           default,   0, "0"
;HKR, NDI\params\BGProtection\enum,      0,         0, %ANTO%
;HKR, NDI\params\BGProtection\enum,      1,         0, %ON%
;HKR, NDI\params\BGProtection\enum,      2,         0, %OFF%

;
; FrameAggregation
;
HKR, ,                            FrameAggregation,0, "1"
;HKR, NDI\params\FrameAggregation,       ParamDesc, 0, %FRAME_AGGREGATION%
;HKR, NDI\params\FrameAggregation,       type,      0, "enum"
;HKR, NDI\params\FrameAggregation,       default,   0, "1"
;HKR, NDI\params\FrameAggregation\enum,  0,         0, %DISABLE%
;HKR, NDI\params\FrameAggregation\enum,  1,         0, %ENABLE%

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
;HKR, NDI\params\IEEE80211H,       ParamDesc,       0, %IEEE80211H%
;HKR, NDI\params\IEEE80211H,       type,            0, "enum"
;HKR, NDI\params\IEEE80211H,       default,         0, "0"
;HKR, NDI\params\IEEE80211H\enum,  0,               0, %DISABLE%
;HKR, NDI\params\IEEE80211H\enum,  1,               0, %ENABLE%

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,      0, "0"
;HKR, NDI\params\AutoChannelSelect,       ParamDesc,0, %AUTO_CH_SELECT%
;HKR, NDI\params\AutoChannelSelect,       type,     0, "enum"
;HKR, NDI\params\AutoChannelSelect,       default,  0, "0"
;HKR, NDI\params\AutoChannelSelect\enum,  0,        0, %DISABLE%
;HKR, NDI\params\AutoChannelSelect\enum,  1,        0, %ENABLE%

;
; SmartScan
;
HKR, ,                               SmartScan,       0, "1"
HKR, NDI\params\SmartScan,           ParamDesc,       0, %SmartScan%
HKR, NDI\params\SmartScan,           type,            0, "enum"
HKR, NDI\params\SmartScan,           default,         0, "0"
HKR, NDI\params\SmartScan\enum,      0,               0, %DISABLE%
HKR, NDI\params\SmartScan\enum,      1,               0, %ENABLE%

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"
HKR, NDI\params\WMMCapable,             ParamDesc, 0, %WMM_CAPABLE%
HKR, NDI\params\WMMCapable,             type,      0, "enum"
HKR, NDI\params\WMMCapable,             default,   0, "1"
HKR, NDI\params\WMMCapable\enum,        0,         0, %DISABLE%
HKR, NDI\params\WMMCapable\enum,        1,         0, %ENABLE%

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "0"
HKR, NDI\params\APSDCapable,            ParamDesc, 0, %APSD_CAPABLE%
HKR, NDI\params\APSDCapable,            type,      0, "enum"
HKR, NDI\params\APSDCapable,            default,   0, "1"
HKR, NDI\params\APSDCapable\enum,       0,         0, %DISABLE%
HKR, NDI\params\APSDCapable\enum,       1,         0, %ENABLE%

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "0"
HKR, NDI\params\APSDAC_BE,              ParamDesc, 0, %AC_BE_APSD%
HKR, NDI\params\APSDAC_BE,              type,      0, "enum"
HKR, NDI\params\APSDAC_BE,              default,   0, "1"
HKR, NDI\params\APSDAC_BE\enum,         0,         0, %DISABLE%
HKR, NDI\params\APSDAC_BE\enum,         1,         0, %ENABLE%

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "0"
HKR, NDI\params\APSDAC_BK,              ParamDesc, 0, %AC_BK_APSD%
HKR, NDI\params\APSDAC_BK,              type,      0, "enum"
HKR, NDI\params\APSDAC_BK,              default,   0, "1"
HKR, NDI\params\APSDAC_BK\enum,         0,         0, %DISABLE%
HKR, NDI\params\APSDAC_BK\enum,         1,         0, %ENABLE%

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "0"
HKR, NDI\params\APSDAC_VI,              ParamDesc, 0, %AC_VI_APSD%
HKR, NDI\params\APSDAC_VI,              type,      0, "enum"
HKR, NDI\params\APSDAC_VI,              default,   0, "1"
HKR, NDI\params\APSDAC_VI\enum,         0,         0, %DISABLE%
HKR, NDI\params\APSDAC_VI\enum,         1,         0, %ENABLE%

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "0"
HKR, NDI\params\APSDAC_VO,              ParamDesc, 0, %AC_VO_APSD%
HKR, NDI\params\APSDAC_VO,              type,      0, "enum"
HKR, NDI\params\APSDAC_VO,              default,   0, "1"
HKR, NDI\params\APSDAC_VO\enum,         0,         0, %DISABLE%
HKR, NDI\params\APSDAC_VO\enum,         1,         0, %ENABLE%

;
; MaxSPLength
;
HKR, ,                            MaxSPLength,     0, "0"
;HKR, Default,                     MaxSPLength,     0, "0"
;HKR, NDI\params\MaxSPLength,      ParamDesc,       0, %MAX_PERIOD_LENGTH%
;HKR, NDI\params\MaxSPLength,      type,            0, "int"
;HKR, Ndi\params\MaxSPLength,      default,         0, "0"
;HKR, NDI\params\MaxSPLength,      min,             0, "0"
;HKR, NDI\params\MaxSPLength,      max,             0, "3"
;HKR, NDI\params\MaxSPLength,      step,            0, "1"
;HKR, NDI\params\MaxSPLength,      optional,        0, "0"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "1"
;HKR, NDI\params\DLSCapable,             ParamDesc, 0, %DLS_CAPABLE%
;HKR, NDI\params\DLSCapable,             type,      0, "enum"
;HKR, NDI\params\DLSCapable,             default,   0, "1"
;HKR, NDI\params\DLSCapable\enum,        0,         0, %DISABLE%
;HKR, NDI\params\DLSCapable\enum,        1,         0, %ENABLE%

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "1"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, %PSP_XLINK%
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "1"
HKR, NDI\params\PSPXlink\enum,    0,               0, %DISABLE%
HKR, NDI\params\PSPXlink\enum,    1,               0, %ENABLE%

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600
;
; Aggressive Roaming
;
;
; Aggressive Roaming
;
HKR, ,                                 CCX2Control,     0x00010001, 0x00fa4600
HKR, ,                                 FstRoam,     0, "0"
HKR, NDI\params\FstRoam,         ParamDesc,          0, %AGGRESSIVE_ROAMING_CONDITION%
HKR, NDI\params\FstRoam,         type,               0, "enum"
HKR, NDI\params\FstRoam,         default,            0, %DISABLE%
HKR, NDI\params\FstRoam\enum,     0,                  0, %DISABLE%
HKR, NDI\params\FstRoam\enum,     1,                  0, %-60DBM%
HKR, NDI\params\FstRoam\enum,     2,                  0, %-70DBM%
HKR, NDI\params\FstRoam\enum,     3,                  0, %-80DBM%
HKR, NDI\params\FstRoam\enum,     4,                  0, %-90DBM%

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%


;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
;HKR, Default,                     NetworkAddress,  0, ""
;HKR, NDI\params\NetworkAddress,   ParamDesc,       0, %MAC_ADDRESS%
;HKR, NDI\params\NetworkAddress,   type,            0, "edit"
;HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
;HKR, NDI\params\NetworkAddress,   default,         0, ""

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, %POWER_SAVING%
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, %CAM%
HKR, NDI\params\PSMode\enum,      1,               0, %MAX_PSP%
HKR, NDI\params\PSMode\enum,      2,               0, %FAST_PSP%

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
;HKR, Default,                     ACPowerCam,      0, "0"
;HKR, NDI\params\ACPowerCam,       ParamDesc,       0, %CAM_AC_POWER%
;HKR, NDI\params\ACPowerCam,       type,            0, "enum"
;HKR, NDI\params\ACPowerCam,       default,         0, "0"
;HKR, NDI\params\ACPowerCam\enum,  0,               0, %DISABLE%
;HKR, NDI\params\ACPowerCam\enum,  1,               0, %ENABLE%

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
;HKR, Default,                     RTSThresh,       0, "2347"
;HKR, NDI\params\RTSThresh,        ParamDesc,       0, %RTS_THRESHOLD%
;HKR, NDI\params\RTSThresh,        type,            0, "int"
;HKR, Ndi\params\RTSThresh,        default,         0, "2347"
;HKR, NDI\params\RTSThresh,        min,             0, "0"
;HKR, NDI\params\RTSThresh,        max,             0, "2347"
;HKR, NDI\params\RTSThresh,        step,            0, "32"
;HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
;HKR, Default,                     FragThresh,      0, "2346"
;HKR, NDI\params\FragThresh,       ParamDesc,       0, %FRAGMENT_THRESHOLD%
;HKR, NDI\params\FragThresh,       type,            0, "int"
;HKR, Ndi\params\FragThresh,       default,         0, "2346"
;HKR, NDI\params\FragThresh,       min,             0, "256"
;HKR, NDI\params\FragThresh,       max,             0, "2346"
;HKR, NDI\params\FragThresh,       step,            0, "32"
;HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""


;*******************************************************************************************
; DeviceID for Win9X 
;*******************************************************************************************
[G122C29x.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_07D1&PID_3C0C"

[G122C19x.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_07D1&PID_3C03"

[WUA13409x.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_07D1&PID_3C04"

[DWA110.ndi.reg]
HKR, Ndi,                         DeviceID,        0, "USB\VID_07D1&PID_3C07"

[USB9X.ndi.reg]
HKR, ,                            NTMPDriver,       0, Dr71WU98.sys

HKR, ,                            BusType,          0, 15
HKR, NDI,                         CardType,         0, "PNP"

HKR, ,                            RunningWin9X,     0, "1"
HKR, ,                            DevLoader,        0, "*ndis"
HKR, ,                            DeviceVxDs,       0, "Dr71WU98.sys"
HKR, ,                            EnumPropPages,    0, "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,              DefUpper,         0, "ndis3"
HKR, Ndi\Interfaces,              DefLower,         0, "ethernet"
HKR, Ndi\Interfaces,              UpperRange,       0, "ndis3"
HKR, Ndi\Interfaces,              LowerRange,       0, "ethernet"

HKR, NDIS,                        LogDriverName,    0, "Dr71WU98"
HKR, NDIS,                        MajorNdisVersion, 1, 03
HKR, NDIS,                        MinorNdisVersion, 1, 0A

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
win9x.CopyFiles         = 11    ; system32 subdirectory on win9x
NTAMD64.CopyFiles   = 12  ; system32\drivers

[NT.CopyFiles]
Dr71WU.sys                   ; NT Installation

[win9x.CopyFiles]
Dr71WU98.sys                     ;  Win9x Installation

[NTAMD64.CopyFiles]
Dr71WU.sys                   ; NT Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
Dr71WU.sys                = 1
Dr71WU98.sys             = 1

[SourceDisksFiles.X86]  
Dr71WU.sys                = 1
Dr71WU98.sys             = 1
 
[SourceDisksFiles.AMD64]
Dr71WU.sys           = 1
Dr71WU98.sys        = 1

 
;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RTUSB.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt73"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[D-Link.Service]
DisplayName                 = %D-Link.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\Dr71WU.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\Dr71WU.sys"
HKR, , TypesSupported,   0x00010001, 7



;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "D-Link Corporation"
D-Link                      = "D-Link Corporation"
DWLG122C2.DeviceDesc        = "D-Link AirPlus G DWL-G122 Wireless USB Adapter(rev.C2)"
DWLG122C1.DeviceDesc        = "D-Link AirPlus G DWL-G122 Wireless USB Adapter(rev.C)"
WUA1340.DeviceDesc          = "D-Link WUA-1340 USB Adapter"
DWA110.DeviceDesc           = "D-Link Wireless G DWA-110 USB Adapter"
INSTALL_DISK_STR            = "D-Link USB Wireless Card Installation Disk"
D-Link.Service.DispName     = "D-Link USB Wireless LAN Card Driver"
;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
SSID_DEF_STR                = "dlink"
VENDOR_DESC_DEF_STR         = "D-Link USB Wireless LAN Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "6"
RADIO_ON_OFF		= "Radio On/Off"
DISABLE			= "Disable"
ENABLE			= "Enable"
AUTO_RECONNECT		= "Auto Reconnect Mode"
COUNTRY_11G		= "Country Region 11G"
CH_1-11			= "(Channel 1 - 11)"
CH_1-13			= "(Channel 1 - 13)"
CH_10-11		= "(Channel 10 - 11)"
CH_10-13		= "(Channel 10 - 13)"
CH_14			= "(Channel 14)"
CH_1-14			= "(Channel 1 - 14)"
CH_3-9			= "(Channel 3 - 9)"
COUNTRY_11A		= "Country Region 11A"
CH_36-64_149-165	= "Ch(36 - 64,149 - 165)"
CH_36-140		= "Ch(36 - 140)"
CH_36-64		= "Ch(36 - 64)"
CH_52-64_149-161	= "Ch(52 - 64,149 - 161)"
CH_149-165		= "Ch(149 - 165)"
CH_149-161		= "Ch(149 - 161)"
CH_36-48		= "Ch(36 - 48)"
CH_36-165		= "Ch(36 - 165)"
CH_52-64		= "Ch(52 - 64)"
CH_34-46		= "Ch(34 - 46)"
CH_34-64		= "Ch(34 - 64)"
ADHOC_MODE		= "Adhoc Wireless Mode"
80211_B_ONLY		= "802.11 B Only"
80211_BG_MIX		= "802.11 B/G Mix"
80211_G_ONLY		= "802.11 G Only"
BG_PROTECTION		= "B/G Protection"
ANTO			= "Auto"
ON			= "On"
OFF			= "Off"
FRAME_AGGREGATION	= "Frame Aggregation"
IEEE80211H		= "IEEE802.11h"
AUTO_CH_SELECT		= "Auto Channel Select"
WMM_CAPABLE		= "WMM Capable"
APSD_CAPABLE		= "APSD Capable"
AC_BE_APSD		= "AC_BE support APSD"
AC_BK_APSD		= "AC_BK support APSD"
AC_VI_APSD		= "AC_VI support APSD"
AC_VO_APSD		= "AC_VO support APSD"
MAX_PERIOD_LENGTH	= "Max Service Period Length"
DLS_CAPABLE		= "DLS Capable"
PSP_XLINK		= "PSP Xlink Mode"
AGGRESSIVE_ROAMING_CONDITION	= "Aggressive Roaming Condition"
-60DBM			= "-60dbm"
-70DBM			= "-70dbm"
-80DBM			= "-80dbm"
-90DBM			= "-90dbm"
MAC_ADDRESS		= "Local Administration MAC Network Address"
POWER_SAVING		= "Power Saving Mode"
CAM			= "CAM (Constantly Awake Mode)"
MAX_PSP			= "Max_PSP (Max Power Savings)"
FAST_PSP		= "Fast_PSP (Power Save Mode)"
CAM_AC_POWER		= "CAM when AC Power"
RTS_THRESHOLD		= "RTS Threshold"
FRAGMENT_THRESHOLD	= "Fragment Threshold"
SmartScan           = "Multimedia/Gaming Environment"