;
; Copyright 2003, Agere Systems Inc
;

[Version]
Signature="$CHICAGO$"
Class=Net
Provider=Agere Systems
DriverVer=01/08/2004, 8.22.50.805
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Compatible=1
;Catalogfile=wlask9x.cat
;Catalogfile.NT=wlask2x.cat

[Manufacturer]
Askey="Askey", NT.5.1
Agere="Agere Systems", NT.5.1
FUJITSU="FUJITSU", NT.5.1

[ControlFlags]
ExcludeFromSelect = *

[Askey]
%N01%=D01,PCMCIA\Askey-IEEE802.11b_Wireless_PC_Card_7008-C194
%N02%=D02,PCMCIA\Askey-IEEE802.11b_Wireless_CF_Card_7009-6843

[Agere Systems]
%N03%=D03,PCI\VEN_11C1&DEV_AB30&SUBSYS_AB3011C1&REV_00
%N04%=D04,PCI\VEN_11C1&DEV_AB34&SUBSYS_AB3411C1&REV_00
%N05%=D05,PCI\VEN_11C1&DEV_AB10&SUBSYS_AB1011C1&REV_01
%N06%=D06,PCMCIA\Agere_Systems-Wireless_PC_Card_Model_0110-C4ED
%N07%=D07,PCMCIA\Agere_Systems-Wireless_PC_Card_Model_0111-595B
%N08%=D08,PCMCIA\Agere_Systems-Wireless_PC_Card_Model_0114-CD2A
%N09%=D09,PCMCIA\Agere_Systems-Wireless_CompactFlash_Card_Model_1401-CD6B

[FUJITSU]
%N10%=D10,PCMCIA\FUJITSU-802.11b_Wireless_LAN_Adapter(A)-4FA9

[Askey.NT.5.1]
%N01%=DXP01,%C01%
%N02%=DXP02,%C02%

[Agere Systems.NT.5.1]
%N03%=DXP03,%C03%
%N04%=DXP04,%C04%
%N05%=DXP05,%C05%
%N06%=DXP06,%C06%
%N07%=DXP07,%C07%
%N08%=DXP08,%C08%
%N09%=DXP09,%C09%

[FUJITSU.NT.5.1]
%N10%=DXP10,%C10%

[D01]
AddReg=AC,A98,A98P2,A98A,A9801
CopyFiles=C98DP2,C98SP2

[A9801]
HKR,,VendorDescription,,%N01%
HKR,Ndi,DeviceID,,%C01%

[D02]
AddReg=AC,A98,A98P2,A98A,A9802
CopyFiles=C98DP2,C98SP2

[A9802]
HKR,,VendorDescription,,%N02%
HKR,Ndi,DeviceID,,%C02%

[D03]
AddReg=AC,A98,AI,A98P2,A98I,A9803
CopyFiles=C98DP2,C98SP2

[A9803]
HKR,,VendorDescription,,%N03%
HKR,Ndi,DeviceID,,%C03%

[D04]
AddReg=AC,A98,AI,A98P2,A98I,A9804
CopyFiles=C98DP2,C98SP2

[A9804]
HKR,,VendorDescription,,%N04%
HKR,Ndi,DeviceID,,%C04%

[D05]
AddReg=AC,A98,AI,A98P2,A98I,A9805
CopyFiles=C98DP2,C98SP2

[A9805]
HKR,,VendorDescription,,%N05%
HKR,Ndi,DeviceID,,%C05%

[D06]
AddReg=AC,A98,A98P2,A98A,A9806
CopyFiles=C98DP2,C98SP2

[A9806]
HKR,,VendorDescription,,%N06%
HKR,Ndi,DeviceID,,%C06%

[D07]
AddReg=AC,A98,A98P2,A98A,A9807
CopyFiles=C98DP2,C98SP2

[A9807]
HKR,,VendorDescription,,%N07%
HKR,Ndi,DeviceID,,%C07%

[D08]
AddReg=AC,A98,A98P2,A98A,A9808
CopyFiles=C98DP2,C98SP2

[A9808]
HKR,,VendorDescription,,%N08%
HKR,Ndi,DeviceID,,%C08%

[D09]
AddReg=AC,A98,A98P2,A98A,A9809
CopyFiles=C98DP2,C98SP2

[A9809]
HKR,,VendorDescription,,%N09%
HKR,Ndi,DeviceID,,%C09%

[D10]
AddReg=AC,A98,A98P2,A98A,A9810
CopyFiles=C98DP2,C98SP2

[A9810]
HKR,,VendorDescription,,%N10%
HKR,Ndi,DeviceID,,%C10%

[D01.NT]
AddReg=AC,A2K,A2KP2,A2K01
CopyFiles=C2KDP2,C2KSP2
Characteristics=0x84
BusType=8

[D01.NT.Services]
AddService=wlask48d,2,SP2,EP2

[D01.NT.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[A2K01]
HKR,,VendorDescription,,%N01%

[D02.NT]
AddReg=AC,A2K,A2KP2,A2K02
CopyFiles=C2KDP2,C2KSP2
Characteristics=0x84
BusType=8

[D02.NT.Services]
AddService=wlask48d,2,SP2,EP2

[D02.NT.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[A2K02]
HKR,,VendorDescription,,%N02%

[D03.NT]
AddReg=AC,A2K,AI,A2KP2,A2K03,A2KI
CopyFiles=C2KDP2,C2KSP2
Characteristics=0x84
BusType=5

[D03.NT.Services]
AddService=wlask48d,2,SP2,EP2

[D03.NT.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[A2K03]
HKR,,VendorDescription,,%N03%

[D04.NT]
AddReg=AC,A2K,AI,A2KP2,A2K04,A2KI
CopyFiles=C2KDP2,C2KSP2
Characteristics=0x84
BusType=5

[D04.NT.Services]
AddService=wlask48d,2,SP2,EP2

[D04.NT.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[A2K04]
HKR,,VendorDescription,,%N04%

[D05.NT]
AddReg=AC,A2K,AI,A2KP2,A2K05,A2KI
CopyFiles=C2KDP2,C2KSP2
Characteristics=0x84
BusType=5

[D05.NT.Services]
AddService=wlask48d,2,SP2,EP2

[D05.NT.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[A2K05]
HKR,,VendorDescription,,%N05%

[D06.NT]
AddReg=AC,A2K,A2KP2,A2K06
CopyFiles=C2KDP2,C2KSP2
Characteristics=0x84
BusType=8

[D06.NT.Services]
AddService=wlask48d,2,SP2,EP2

[D06.NT.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[A2K06]
HKR,,VendorDescription,,%N06%

[D07.NT]
AddReg=AC,A2K,A2KP2,A2K07
CopyFiles=C2KDP2,C2KSP2
Characteristics=0x84
BusType=8

[D07.NT.Services]
AddService=wlask48d,2,SP2,EP2

[D07.NT.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[A2K07]
HKR,,VendorDescription,,%N07%

[D08.NT]
AddReg=AC,A2K,A2KP2,A2K08
CopyFiles=C2KDP2,C2KSP2
Characteristics=0x84
BusType=8

[D08.NT.Services]
AddService=wlask48d,2,SP2,EP2

[D08.NT.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[A2K08]
HKR,,VendorDescription,,%N08%

[D09.NT]
AddReg=AC,A2K,A2KP2,A2K09
CopyFiles=C2KDP2,C2KSP2
Characteristics=0x84
BusType=8

[D09.NT.Services]
AddService=wlask48d,2,SP2,EP2

[D09.NT.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[A2K09]
HKR,,VendorDescription,,%N09%

[D10.NT]
AddReg=AC,A2K,A2KP2,A2K10
CopyFiles=C2KDP2,C2KSP2
Characteristics=0x84
BusType=8

[D10.NT.Services]
AddService=wlask48d,2,SP2,EP2

[D10.NT.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[A2K10]
HKR,,VendorDescription,,%N10%

[DXP01]
AddReg=AC,AXP,AXPP2,AXP01
DelReg=DRXPV
CopyFiles=CXPDP2,CXPSP2
Characteristics=0x84
BusType=8

[DXP01.Services]
AddService=wlask48d,2,SP2,EP2

[DXP01.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[AXP01]
HKR,,VendorDescription,,%N01%

[DXP02]
AddReg=AC,AXP,AXPP2,AXP02
DelReg=DRXPV
CopyFiles=CXPDP2,CXPSP2
Characteristics=0x84
BusType=8

[DXP02.Services]
AddService=wlask48d,2,SP2,EP2

[DXP02.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[AXP02]
HKR,,VendorDescription,,%N02%

[DXP03]
AddReg=AC,AXP,AI,AXPP2,AXP03,AXPI
DelReg=DRXPV
CopyFiles=CXPDP2,CXPSP2
Characteristics=0x84
BusType=5

[DXP03.Services]
AddService=wlask48d,2,SP2,EP2

[DXP03.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[AXP03]
HKR,,VendorDescription,,%N03%

[DXP04]
AddReg=AC,AXP,AI,AXPP2,AXP04,AXPI
DelReg=DRXPV
CopyFiles=CXPDP2,CXPSP2
Characteristics=0x84
BusType=5

[DXP04.Services]
AddService=wlask48d,2,SP2,EP2

[DXP04.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[AXP04]
HKR,,VendorDescription,,%N04%

[DXP05]
AddReg=AC,AXP,AI,AXPP2,AXP05,AXPI
DelReg=DRXPV
CopyFiles=CXPDP2,CXPSP2
Characteristics=0x84
BusType=5

[DXP05.Services]
AddService=wlask48d,2,SP2,EP2

[DXP05.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[AXP05]
HKR,,VendorDescription,,%N05%

[DXP06]
AddReg=AC,AXP,AXPP2,AXP06
DelReg=DRXPV
CopyFiles=CXPDP2,CXPSP2
Characteristics=0x84
BusType=8

[DXP06.Services]
AddService=wlask48d,2,SP2,EP2

[DXP06.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[AXP06]
HKR,,VendorDescription,,%N06%

[DXP07]
AddReg=AC,AXP,AXPP2,AXP07
DelReg=DRXPV
CopyFiles=CXPDP2,CXPSP2
Characteristics=0x84
BusType=8

[DXP07.Services]
AddService=wlask48d,2,SP2,EP2

[DXP07.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[AXP07]
HKR,,VendorDescription,,%N07%

[DXP08]
AddReg=AC,AXP,AXPP2,AXP08
DelReg=DRXPV
CopyFiles=CXPDP2,CXPSP2
Characteristics=0x84
BusType=8

[DXP08.Services]
AddService=wlask48d,2,SP2,EP2

[DXP08.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[AXP08]
HKR,,VendorDescription,,%N08%

[DXP09]
AddReg=AC,AXP,AXPP2,AXP09
DelReg=DRXPV
CopyFiles=CXPDP2,CXPSP2
Characteristics=0x84
BusType=8

[DXP09.Services]
AddService=wlask48d,2,SP2,EP2

[DXP09.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[AXP09]
HKR,,VendorDescription,,%N09%

[DXP10]
AddReg=AC,AXP,AXPP2,AXP10
DelReg=DRXPV
CopyFiles=CXPDP2,CXPSP2
Characteristics=0x84
BusType=8

[DXP10.Services]
AddService=wlask48d,2,SP2,EP2

[DXP10.CoInstallers]
CopyFiles=CCIP2
AddReg=ACIP2

[AXP10]
HKR,,VendorDescription,,%N10%

[S]
HKR,,Silent,,"0"

[AC]
HKR,,DriverMajor,,"8"
HKR,,DriverMinor,,"22"
HKR,,DriverEnable,,"1"
HKR,,Configured,,"1"
HKR,,DesiredSSID,,"Agere Systems"
HKR,Ndi\Interfaces,LowerRange,0,"ethernet"

[AI]
HKR, Ndi\params\PCI_WOL,default,2,0
HKR, Ndi\params\PCI_WOL,type,0,enum
HKR, Ndi\params\PCI_WOL\enum,"0",0,%OFF%
HKR, Ndi\params\PCI_WOL\enum,"1",0,%ON%

[A98]
HKR,,LoadVxD,,1
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR,,IOBaseAddress,1,02,00,00,00
HKR,,InterruptNumber,1,04,00,00,00
HKR,,EnableIRQSharing,1,01,00,00,00
HKR,,OSType,,"2"
HKR,Ndi\Interfaces,DefLower,0,"ethernet"
HKR,Ndis,MajorNdisVersion,1,03
HKR,Ndis,MinorNdisVersion,1,0A

[A98P2]
HKR,,DriverVariant,,"3"
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,wlask48c.sys
HKR,Ndi\Interfaces,DefUpper,0,"ndis3"
HKR,Ndi\Interfaces,UpperRange,0,"ndis3"
HKR,Ndi,NdiInstaller,,"wiask48c.dll,WV41NdiProc"
HKR,Ndis,LogDriverName,,"wlask48c"

[A98A]
HKR,,BusType,,8
HKR,Ndi,CardType,,"PCMCIA"

[A98I]
HKR,,BusType,,5
HKR,Ndi,CardType,,"PCI"
HKR, Ndi\params\PCI_WOL,ParamDesc,0,%WOL%

[A2K]
HKR,Ndi\Interfaces,UpperRange,0,"ndis5"
HKR,,NDT,,"1"
HKR,,OSType,,"8"

[A2KP2]
HKR,,DriverVariant,,"4"
HKR,Ndi,Service,0,"wlask48d"

[A2KI]
HKR, Ndi\params\PCI_WOL,ParamDesc,0,%WOL%

[AXP]
HKR,,NDT,,"1"
HKR,,OSType,,"32"
HKR,Ndi\Interfaces,UpperRange,0,"ndis5"
HKR,Ndi\params\OwnChannel,ParamDesc,0,%1CH%
HKR,Ndi\params\OwnChannel,Type,0,enum
HKR,Ndi\params\OwnChannel,Default,0, 0
HKR,Ndi\params\OwnChannel\enum,0,0,%UD%
HKR,Ndi\params\OwnChannel\enum,1,0,"01"
HKR,Ndi\params\OwnChannel\enum,2,0,"02"
HKR,Ndi\params\OwnChannel\enum,3,0,"03"
HKR,Ndi\params\OwnChannel\enum,4,0,"04"
HKR,Ndi\params\OwnChannel\enum,5,0,"05"
HKR,Ndi\params\OwnChannel\enum,6,0,"06"
HKR,Ndi\params\OwnChannel\enum,7,0,"07"
HKR,Ndi\params\OwnChannel\enum,8,0,"08"
HKR,Ndi\params\OwnChannel\enum,9,0,"09"
HKR,Ndi\params\OwnChannel\enum,10,0,"10"
HKR,Ndi\params\OwnChannel\enum,11,0,"11"
HKR,Ndi\params\OwnChannel\enum,12,0,"12"
HKR,Ndi\params\OwnChannel\enum,13,0,"13"
HKR,Ndi\params\OwnChannel\enum,14,0,"14"
HKR,Ndi\params\PowerMode,ParamDesc,0,%2PM%
HKR,Ndi\params\PowerMode,Type,0,enum
HKR,Ndi\params\PowerMode,Default,0,0
HKR,Ndi\params\PowerMode\enum,2,0,%AUTO%
HKR,Ndi\params\PowerMode\enum,1,0,%ON%
HKR,Ndi\params\PowerMode\enum,0,0,%OFF%

[AXPP2]
HKR,,DriverVariant,,"4"
HKR,Ndi,Service,0,"wlask48d"

[AXPI]
HKR, Ndi\params\PCI_WOL,ParamDesc,0,%3WOL%

[C98DP2]
wlask48c.sys

[C2KDP2]
wlask48d.sys

[CXPDP2]
wlask48d.sys

[C98SP2]
wcask48c.exe
waask48c.dll
wnask48c.cpl
wnask.hlp
wnask.cnt
wuask48c.vxd
wiask48c.dll

[C2KSP2]
wcask48d.exe
waask48d.dll
wnask48d.cpl
wnask.hlp
wnask.cnt

[CXPSP2]
wcask48d.exe
waask48d.dll
wnask48d.cpl
wnask.hlp
wnask.cnt

[ACIP2]
HKR,,CoInstallers32,0x00010000,"wdask48d.dll,WLDeviceCoInstaller"

[CCIP2]
wdask48d.dll

[DRXPV]
HKR,Ndi\params

[SP2]
DisplayName=%SDP2%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\wlask48d.sys
LoadOrderGroup=NDIS

[EP2]
AddReg=ALP2

[ALP2]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\wlask48d.sys"
HKR,,TypesSupported,0x00010001,7

[DestinationDirs]
DefaultDestDir=11
C98DP2=11
C2KDP2=12
CXPDP2=12
CCIP2=11
C98SP=11
C98SU=11
C2KSP=11
C2KSU=11
CXPSP=11
CXPSU=11
CCIP=11
CCIU=11

[SourceDisksNames]
1 = %DISKID%,,,

[SourceDisksFiles]
wlask48c.sys=1
wlask48d.sys=1
wcask48c.exe=1
wcask48d.exe=1
waask48c.dll=1
waask48d.dll=1
wdask48d.dll=1
wnask48c.cpl=1
wnask48d.cpl=1
wuask48c.vxd=1
wiask48c.dll=1
wnask.hlp=1
wnask.cnt=1

[Strings]
1CH="1. Channel"
2PM="2. Card Power Management"
3WOL="3. Wake On Lan"
WOL="Wake On Lan"
UD="Use default channel"
OFF="Off"
ON="On"
AUTO="Auto"

DISKID="Wireless Disk"

N01="IEEE802.11b Wireless PC Card 7008"
N02="IEEE802.11b Wireless CF Card 7009"

N03="Wireless Mini PCI Card Model 0506"
N04="Wireless Mini PCI Card Model 0508"
N05="Wireless Mini PCI Card Model 0509"
N06="Wireless PC Card Model 0110"
N07="Wireless PC Card Model 0111"
N08="Wireless PC Card Model 0114"
N09="Wireless CompactFlash Card Model 1401"

N10="802.11b Wireless LAN Adapter(A)"

C01="PCMCIA\Askey-IEEE802.11b_Wireless_PC_Card_7008-C194"
C02="PCMCIA\Askey-IEEE802.11b_Wireless_CF_Card_7009-6843"

C03="PCI\VEN_11C1&DEV_AB30&SUBSYS_AB3011C1&REV_00"
C04="PCI\VEN_11C1&DEV_AB34&SUBSYS_AB3411C1&REV_00"
C05="PCI\VEN_11C1&DEV_AB10&SUBSYS_AB1011C1&REV_01"
C06="PCMCIA\Agere_Systems-Wireless_PC_Card_Model_0110-C4ED"
C07="PCMCIA\Agere_Systems-Wireless_PC_Card_Model_0111-595B"
C08="PCMCIA\Agere_Systems-Wireless_PC_Card_Model_0114-CD2A"
C09="PCMCIA\Agere_Systems-Wireless_CompactFlash_Card_Model_1401-CD6B"

C10="PCMCIA\FUJITSU-802.11b_Wireless_LAN_Adapter(A)-4FA9"

SDP2="802.11b WLAN PC Card Service"
