;OIISER.VXD

[version]
LayoutFile= Layout.inf, Layout1.inf, Layout2.inf
signature="$CHICAGO$"
Class=Ports
ClassGUID={4d36e978-e325-11ce-bfc1-08002be10318}
Provider="FUJITSU"

[ClassInstall]
AddReg=PortsClass.AddReg

[PortsClass.AddReg]
HKR,,,,"Ports (COM & LPT)"
HKR,,Icon,,-23

[Manufacturer]
"FUJITSU"

[FUJITSU]
"FUJITSU Bluetooth Card (UART)" = ComPort, MF\FJUART

[ComPort]
AddReg=ComPort.AddReg
LogConfig=c14,c1a,c23,c2a,c34,c3a,c43,c4a,caa

[ComPort.AddReg]
HKR,,DevLoader,,*vcomm
;HKR,,Enumerator,,serenum.vxd
HKR,,PortDriver,2,oiiser.vxd
HKR,,Contention,,*vcd
HKR,,ConfigDialog,,serialui.dll
HKR,,DCB,3,1C,00,00,00, 80,25,00,00, 11,33,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,PortSubClass,1,01
HKR,,EnumPropPages,,"serialui.dll,EnumPropPages"

; The following sections are COM port resource configs.
; Section name format means:
; Char 1 = c (COM port)
; Char 2 = I/O config: 1 (3f8), 2 (2f8), 3 (3e8), 4 (2e8), a (any)
; Char 3 = IRQ config: #, a (any)

[c14]                   ; COM1,IRQ4
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::)
IRQConfig=S:4

[c1a]                   ; COM1, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=3f8-3ff(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[c23]                   ; COM2, IRQ3
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=S:3

[c2a]                   ; COM2, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=2f8-2ff(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[c34]                   ; COM3, IRQ4
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=S:4

[c3a]                   ; COM3, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=3e8-3ef(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[c43]                   ; COM4, IRQ3
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=S:3,5

[c4a]                   ; COM4, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=2e8-2ef(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15

[caa]                   ; Any base, any IRQ
ConfigPriority=HARDRECONFIG
IOConfig=8@100-ffff%fff8(3ff::)
IRQConfig=S:3,4,5,7,9,10,11,12,14,15
